| CustomiOSApi 1.09

PrinterFeatures.h
1//
2// PrinterFeatures.h
3// CustomiOSApi
4//
5// Created by sviluppo on 29/10/15.
6// Copyright © 2015 Custom Engineering. All rights reserved.
7//
8
9#import <Foundation/Foundation.h>
10
11//Hide it in the documentation
12// @cond PRIVATE
13@interface PrinterFeatures : NSObject
14{
15@public
16
17@protected
18
19@private
20 Boolean statusFEAT_ITF_RS232;
21 Boolean statusFEAT_ITF_USB;
22 Boolean statusFEAT_ITF_ETH;
23 Boolean statusFEAT_ITF_BLUETOOTH;
24 Boolean statusFEAT_ITF_WIFI;
25 Boolean statusFEAT_ITF_IRDA;
26 Boolean statusFEAT_ITF_CENTRONICS;
27 Boolean statusFEAT_SENS_PAPER;
28 Boolean statusFEAT_SENS_NOTCH ;
29 Boolean statusFEAT_SENS_PAPOUT;
30 Boolean statusFEAT_SENS_CUTTER;
31 Boolean statusFEAT_SENS_PAP_NOTCH;
32 Boolean statusFEAT_SENS_NPE;
33 Boolean statusFEAT_MEC_CUTTER;
34 Boolean statusFEAT_MEC_EJECTER;
35 Boolean statusFEAT_MEC_FEEDER;
36 Boolean statusFEAT_MEC_STACKER;
37 Boolean statusFEAT_MEC_ANTIJAM;
38 Boolean statusFEAT_MEC_REWINDER;
39 Boolean statusFEAT_MEC_SELECTOR;
40 Boolean statusFEAT_MEC_GUIDE6SENS;
41 Boolean statusFEAT_ADDIN_BCREADER;
42 Boolean statusFEAT_ADDIN_RFID;
43 Boolean statusFEAT_ADDIN_CHIPCARD;
44 Boolean statusFEAT_ADDIN_SD_MMC;
45 Boolean statusFEAT_ADDIN_LCD;
46 Boolean statusFEAT_ADDIN_DIPSWITCH ;
47 Boolean statusFEAT_SW_BARCODEC2D;
48 Boolean statusFEAT_SW_TRUETYPE;
49 Boolean statusFEAT_SW_VERYNOTCH;
50 Boolean statusFEAT_SW_VERIPRINT;
51 Boolean statusFEAT_SW_BICOLOR;
52 Boolean statusFEAT_SW_MASSSTORAGE;
53 Boolean statusFEAT_SW_FONT_BIG5 ;
54 Boolean statusFEAT_SW_FONT_GB2312;
55 Boolean statusFEAT_DESC_POS;
56 Boolean statusFEAT_DESC_300dpi;
57 Boolean statusFEAT_GUIDE_KPM302;
58 Boolean statusFEAT_MEC_ANNULLO;
59 Boolean statusFEAT_TOP_NOTCH;
60 Boolean statusFEAT_AERO;
61 Boolean statusFEAT_GRAYSCALE_4BIT;
62}
63
64-(id)initWithBuffer:(NSData*)bBufferData;
65
66-(Boolean) StsFEAT_ITF_RS232;
67-(Boolean) StsFEAT_ITF_USB;
68-(Boolean) StsFEAT_ITF_ETH;
69-(Boolean) StsFEAT_ITF_BLUETOOTH;
70-(Boolean) StsFEAT_ITF_WIFI;
71-(Boolean) StsFEAT_ITF_IRDA;
72-(Boolean) StsFEAT_ITF_CENTRONICS;
73-(Boolean) StsFEAT_SENS_PAPER;
74-(Boolean) StsFEAT_SENS_NOTCH ;
75-(Boolean) StsFEAT_SENS_PAPOUT;
76-(Boolean) StsFEAT_SENS_CUTTER;
77-(Boolean) StsFEAT_SENS_PAP_NOTCH;
78-(Boolean) StsFEAT_SENS_NPE;
79-(Boolean) StsFEAT_MEC_CUTTER;
80-(Boolean) StsFEAT_MEC_EJECTER;
81-(Boolean) StsFEAT_MEC_FEEDER;
82-(Boolean) StsFEAT_MEC_STACKER;
83-(Boolean) StsFEAT_MEC_ANTIJAM;
84-(Boolean) StsFEAT_MEC_REWINDER;
85-(Boolean) StsFEAT_MEC_SELECTOR;
86-(Boolean) StsFEAT_MEC_GUIDE6SENS;
87-(Boolean) StsFEAT_ADDIN_BCREADER;
88-(Boolean) StsFEAT_ADDIN_RFID;
89-(Boolean) StsFEAT_ADDIN_CHIPCARD;
90-(Boolean) StsFEAT_ADDIN_SD_MMC;
91-(Boolean) StsFEAT_ADDIN_LCD;
92-(Boolean) StsFEAT_ADDIN_DIPSWITCH ;
93-(Boolean) StsFEAT_SW_BARCODEC2D;
94-(Boolean) StsFEAT_SW_TRUETYPE;
95-(Boolean) StsFEAT_SW_VERYNOTCH;
96-(Boolean) StsFEAT_SW_VERIPRINT;
97-(Boolean) StsFEAT_SW_BICOLOR;
98-(Boolean) StsFEAT_SW_MASSSTORAGE;
99-(Boolean) StsFEAT_SW_FONT_BIG5 ;
100-(Boolean) StsFEAT_SW_FONT_GB2312;
101-(Boolean) StsFEAT_DESC_POS;
102-(Boolean) StsFEAT_DESC_300dpi;
103-(Boolean) StsFEAT_GUIDE_KPM302;
104-(Boolean) StsFEAT_MEC_ANNULLO;
105-(Boolean) StsFEAT_TOP_NOTCH;
106-(Boolean) StsFEAT_AERO;
107-(Boolean) StsFEAT_GRAYSCALE_4BIT;
108
109@end